英语
/*CH1 control */
/*CH2 control */
/*CH3 control */
/*CH4 control */
/*CH5 control */
/*CH6 control */
/*CH7 control */
/*CH8 control */
/*Timer            ON     */
/*Timer            pause   */
/*Timer            reset   */
/*4WS type     (front)    */
/*4WS type    (reverse)  */
/*4WS type       (same)  */
/*4WS type       (rear)    */
/*Dual ESC      (front)    */
/*Dual ESC       (4WD)   */
/*Dual ESC       (rear)    */
/*Gyro gain                */
/*Gyro gain group      */
/*CH1             */
/*CH2             */
/*CH3             */
/*CH4             */
/*CH5             */
/*CH6             */
/*CH7             */
/*CH8             */
/*         ON   */
/*        OFF   */
/*Cancel */
/*Previous */
/*Next */
/*Reset */
/*← */
/*→ */
/*Delete */
/*Cancel */
/*Confirm */
/*Model rename */
/*User name rename */
/*Model */
/*Low Battery Voltage */
/*Snapshot Successfully! */
/*System */
/*Tools */
/*Basics */
/*Telemetry */
/*Curve */
/*Mixing setting */
/*Model */
/*SD card */
/*Info */
/*Home */
/*ST Trim */
/*TH Trim */
/*Trim/Dial */
/*Telemetry */
/*Receiver voltage */
/*Engine battery voltage */
/*RPM */
/*Temperature */
/*RSSI signal */
/*℃ */
/*Channel */
/*Servo view  */
/*Value */
/*Timers */
/*Telemetry */
/*Key */
/*Function */
/*State */
/*System menu */
/*Language*/
/*Desktop setting */
/*Theme setting */
/*Backlight */
/*Sound */
/*Battery */
/*Vibration setting */
/*LED setting */
/*External input output */
/*HOME button setting */
/*Calibration */
/*Tools menu */
/*Trim/Dial select */
/*Switch select */
/*Screenshot setting */
/*Timer */
/*Lap list */
/*Roll out chart */
/*Gear ratio chart */
/*Basic menu */
/*Receiver setting */
/*Servo view */
/*Throttle setting(Trigger) */ 
/*Channel reverse */
/*Sub trim */
/*end point */
/*Fail-safe */
/*Acceleration */
/*Condition */
/*Idle up */
/*Double ratio*/
/*Channel limiter */
/*Channel setting */
/*Telemetry setting */
/*Sensor list */
/*Sensor setting */
/*Telemetry broadcast*/
/*Racing menu*/
/*Steering curve */
/*Throttle curve */
/*Brake curve */
/*Steering delay */
/*Throttle delay */
/*Traction control */
/*A.B.S. */
/*Motor Start */
/*Engine cut */
/*Mixing setting*/
/*Steering mixing */
/*Brake mixing */
/*Gyro mixing */
/*4WS mixing */
/*Dual ESC mixing */
/*CPS mixing */
/*Tank mixing */
/*Programmable mixing */
/*Tilt mixing */
/*Model select */
/*SD card */
/*Information */
/*Model select */
/*Previous */
/*Next */
/*” ” */
/*Model select */
/*Copy model */
/*Paste model */
/*Delete model */
/*Rename */
/*Reset */
/*Cancel */
/*Are you sure to select the model? */
/*Are you sure to copy the model? */
/*Copy */
/*to */
/*Are you sure to delete the data? */
/*Are you sure to rename the model? */
/*Are you sure to reset the model? */
/*The model you are using */
/*Inhibit delete */
/*Copy data error */
/*Please copy again */
/*Confirm */
/*Cancel */
/*Information */
/*User name */
/*Language */
/* */
/* */
/* */
/* */
/* */
/* */
/* */
/* */
/*Factory data reset */
"/*It will reset and delete
all the model settings.
Are you sure to reset
the factory data? */"
/*Confirm */
/*Cancel */
/*Reset system settings */
/*Are you sure to reset system settings？ */
/*NULL */
/*CH1 */
/*CH2 */
/*CH3 */
/*CH4 */
/*CH5 */
/*CH6 */
/*CH7 */
/*CH8 */
/*NULL */
/*DT1 */
/*DT2 */
/*DT3 */
/*DT4 */
/*DL1 */
/*NULL */
/*PS1 */
/*PS2 */
/*PS3 */
/*PS4 */
/*PS5 */
/*Steering */
/*Trigger */
/*NULL */
/*Sound */
/*Warning1 */
/*Warning2 */
/*Warning3 */
/*Warning4 */
/*Warning5 */
/*Warning6 */
/*Warning7 */
/*Warning8 */
/*Warning9 */
/*Warning10 */
/*Warning11 */
/*Warning12 */
/*Warning13 */
/*Warning14 */
/*Warning15 */
/*Warning16 */
/*Warning17 */
/*Warning18 */
/*Warning19 */
/*Warning20 */
/*Confirm */
/*Cancel */
/*Backlight setting */
/*Backlight */
/*Always on */
/*Decrease */
/*Decrease time */
/*Switch */
/*INH */
/*Sound setting */
/*Sound */
/*Other setting */
/*Voice mode */
/*Normal volume */
/*Warning volume */
/*Voice volume */
/*Duration */
/*Frequency + */
/*Press button to broadcast */
/*All */
/*Without key tone */
/*Alarm only */
/*Silence */
/*Only newest content */
/*The 1st & last operate content */
/*All the content */
/*Transmitter voltage */
/*Voltage */
/*Current voltage */
/*Calibrate */
/*Minimum */
/*Maximum */
/*Alarm voltage */
/*Alarm sound */
/*Interval */
/*Auto OFF */
/*Voltage */
/*Type1 */
/*Year */
/*Month */
/*Day */
/*Hour */
/*Minute */
/*Second */
/*Date/Time */
/*Date */
/*Time */
/*Total time */
/*Display mode */
/*Reset */
/*Total time */
/*Date/Time */
/*Total time */
/*LED setting */
/*Brightness */
/*LED type */
/*Always on */
/*Breathe */
/*Backlight */
/*OFF */
/*Calibration */
/*Wheel */
/*Trigger */
/*Rotary knob */
/*End point */
/*End point */
/*End point */
/*Touch test */
/*Click to exit the test */
/*Calibrating... */
"/*Trigger/Wheel/Rotary 
knob calibrate steps:   

1.to maximum  
2.to minimum  
3.to neutral  
4.Wait for the value to stabilize
5.click ”calibration finished”   */"
/*Wheel/Trigger/Rotary knob */
/*Minimum */
/*Neutral */
/*Maximum */
/*Calibration finished */
/*Pink */
/*Yellow */
/*Green */
/*Cyan */
/*Gray */
/*Black */
/*White */
/*Customized */
/*Cancel */
/*Secondary color */
/*Red */
/*Green */
/*Blue */
/*Confirm */
/*Cancel */
/*Desktop setting */
/*Touch timing */
/*theme setting */
/*Built-in theme */
/*Theme 1 */
/*Theme 2 */
/*Theme 3 */
/*Theme 4 */
/*Theme 5 */
/*Custom theme */
/*Theme */
/*Background */
/*Font */
/*SET */
/*CH1 occupied */
/*CH2 occupied */
/*CH3 occupied */
/*CH4 occupied */
/*CH5 occupied */
/*CH6 occupied */
/*CH7 occupied */
/*CH8 occupied */
/*NULL */
/*Steering trim */
/*Throttle trim */
/*Rotary knob trim */
/*Flap */
/*Ratio Switch*/
/*Sub trim CH1 */
/*Sub trim CH2 */
/*Sub trim CH3 */
/*Sub trim CH4 */
/*Sub trim CH5 */
/*Sub trim CH6 */
/*Sub trim CH7 */
/*Sub trim CH8 */
/*Acceleration(forward) */
/*Acceleration(brake1) */
/*Acceleration(brake2) */
/*Acceleration(brake3) */
/*Steering curve */
/*Throttle curve */
/*ST delay(turn) */
/*ST delay(return) */
/*TH delay(turn/high) */
/*TH delay(turn/middle) */
/*TH delay(turn/low) */
/*TH delay(return/high) */
/*TH delay(return/middle) */
/*TH delay(return/low) */
/*ABS(return brake1) */
/*ABS(delay brake1) */
/*ABS(cycle brake1) */
/*ABS(return brake2) */
/*ABS(delay brake2) */
/*ABS(cycle brake2) */
/*ABS(return brake3) */
/*ABS(delay brake3) */
/*ABS(cycle brake3) */
/*Traction control(return) */
/*Traction control(delay) */
/*Traction control(cycle) */
/*Brake rate(brake1) */
/*Brake EXP(brake1) */
/*Brake delay(brake1) */
/*Brake rate(brake2) */
/*Brake EXP(brake2) */
/*Brake delay(brake2) */
/*Brake rate(brake3) */
/*Brake EXP(brake3) */
/*Brake delay(brake3) */
/*Brake2,3ratio*/
/*Tilt mixing(RUD->FLP) */
/*Tilt mixing(FLP->RUD) */
/*Idle up */
/*Prog. mixing1 A */
/*Prog. mixing1 B */
/*Prog. mixing2 A */
/*Prog. mixing2 B */
/*Prog. mixing3 A */
/*Prog. mixing3 B */
/*Prog. mixing4 A */
/*Prog. mixing4 B */
/*Prog. mixing5 A */
/*Prog. mixing5 B */
/*Prog. mixing6 A */
/*Prog. mixing6 B */
/*Prog. mixing7 A */
/*Prog. mixing7 B */
/*Prog. mixing8 A */
/*Prog. mixing8 B */
/*4WS front rate */
/*4WS rear rate */
/*Dual ESC */
/*Dual ESC ratio */
/*Gyro gain */
/*Ackermann */
/*Condition */
/*End point switch */
/*Brake ratio */
/*Cruise ratio */
/*Trim/Dial select */
/*Function */
/*Dir. */
/*Step */
/*Nor. */
/*Rev. */
/*Buzzer */
/*Warning voice */
/*System voice */
/*Customized voice */
/*Auto */
/*NONE */
/*Beep1 */
/*Beep2 */
/*Beep3 */
/*Beep4 */
/*Beep5 */
/*Beep6 */
/*Beep7 */
/*Beep8 */
/*Warning1 */
/*Warning2 */
/*Warning3 */
/*Warning4 */
/*Warning5 */
/*Warning6 */
/*Warning7 */
/*Warning8 */
/*Warning9 */
/*Warning10 */
/*Warning11 */
/*Warning12 */
/*Warning13 */
/*Warning14 */
/*Warning15 */
/*Warning16 */
/*Warning17 */
/*Warning18 */
/*Warning19 */
/*Warning20 */
/*Key tone setting */
/*Audio source */
/*Buzzer */
/*Audition */
/*Stop audition */
/*NULL */
/*Condition1<-->2 */
/*Condition1 */
/*Condition2 */
/*Condition3 */
/*Condition4 */
/*Program. mixing1 */
/*Program. mixing2 */
/*Program. mixing3 */
/*Program. mixing4 */
/*Program. mixing5 */
/*Program. mixing6 */
/*Program. mixing7 */
/*Program. mixing8 */
/*A.B.S(brake1) */
/*A.B.S(brake2) */
/*A.B.S(brake3) */
/*Traction control */
/*4WS type switching */
/*4WS type1(front) */
/*4WS type2(reverse) */
/*4WS type3(same) */
/*4WS type4(rear) */
/*Dual ESC(front) */
/*Dual ESC(4WD) */
/*Dual ESC(rear) */
/*Gyro mixing */
/*Gyro gain */
/*Gyro gain group */
/*CPS mixing1 */
/*CPS mixing2 */
/*CPS mixing3 */
/*CPS mixing4 */
/*Brake */
/*Motor Start */
/*Engine cut */
/*Idle up */
/*Neutral brake */
/*Timer start */
/*Timer reset */
/*Screen capture */
/*Backlight */
/*Telemetry broadcast*/
/*Stop speech */
/*End point switch */
/*Cruise control */
/*Ratio Switch*/
/*Switch select */
/*Function */
/*Dir. */
/*Type */
/*Steering switch(SS) */
/*Trigger switch(TS) */
/*Nor. */
/*Rev. */
/*jog */
/*lock */
/*Sound setting */
/*Audio source */
/*System voice */
/*Stop audition */
/*System menu */
/*User menu */
/*Trim lock */
/*Model select */
/*Channel reverse */
/*Sub trim */
/*End point adjustment */
/*Throttle curve */
/*Steering curve */
/*Brake curve */
/*Speed */
/*Fail-safe */
/*Receiver select */
/*Model menu */
/*Traction control */
/*A.B.S. */
/*Acceleration */
/*Idle up */
/*Engine cut */
/*throttle start */
/*Steering mixting */
/*Brake mixing */
/*Program. mixing */
/*Gyro mixing */
/*4WS mixing */
/*CPS mixing */
/*Tank mixing */
/*Tilt mixing */
/*Dual ESC */
/*Channel limiter */
/*S.BUS gyro */
/*ESC connect */
/*Timer */
/*Lap list */
/*Roll out chart */
/*Gear ratio chart */
/*System menu */
/*Trim select */
/*Switch select */
/*Throttle setting */
/*Channel select */
/*Double ratio*/
/*Condition */
/*Servo review */
/*Telemetry */
/*Sensor list */
/*Sensor menu */
/*Data reset */
/*HOME button select */
/*Push */
/*Long press */
/*User menu */
/*Power on/off */
/*External input output */
/*protocol output mode */
/*Multimedia Mode */
/*USB power output */
/*pop-up window */
/*Audio output */
/*Video input */
/*Close */
/*Open */
/*Auto */
/*Vibration setting */
/*Vibration by touch */
/*Touch sense */
/*Warning sense */
/*Vibration */
/*Screenshot select */
/*Switch */
"/*Attention!
Screenshots will take 3 to 5 seconds, the display will stop refreshing and the memory card will not be pluggable  */"
/*Timer setup */
/*Timer */
/*Current time */
/*Alarm time */
/*Mode */
/*Voice */
/*Start */
/*Reset */
/*Other */
/*Vibrator */
/*throttle trigger */
/*Up timer */
/*Type1 */
/*Type1 */
/*Desktop click timer*/
/*Up timer */
/*Fuel down timer */
/*Lap timer */
/*Lap navigate timer */
/*NULL */
/*Type1 */
/*Type2 */
/*Type3 */
/*Lap list */
/*Total */
/*Average */
/*Reset */
/*Roll out chart */
/*Pinion */
/*Spur */
/*Diameter */
/*Step */
/*Gear ratio chart */
/*Pinion */
/*Spur */
/*2nd gear ratio */
/*Receiver setting */
/*Subsidiary ID mode*/
/*Subsidiary ID */
"/* Replacing the receiver protocol requires re-binding
Do you confirm? */"
/*Receivers List */
/*Receivers List */
/*protocol selection */
/*Subsidiary ID setting */
"/*Hint:
FHSS V1 protocol PWM output resolution level is 2048. 

FHSS V2 protocol PWM output resolution level is 4096, FHSS V2 can achieve a more precise operation.(R8FG_V1.0 does not support FHSS V2 protocol)*/"
/*Servo view */
/*Trigger setting*/
/*Ratio */
/*Neutral brake */
/*Brake rate */
/*Switch */
/*Forward 100: Brake 0 */
/*Cruise control */
/*Throttle rate */
/*Tune Buttons  */
/*Forward 50: Brake 50 */
/*Forward 70: Brake 30 */
/*Forward 100: Brake 0 */
/*Channel reverse */
/*Channel 1   */
/*Channel 2   */
/*Channel 3   */
/*Channel 4   */
/*Channel 5   */
/*Channel 6   */
/*Channel 7   */
/*Channel 8   */
/*Sub trim */
/*Channel 1   */
/*Channel 2   */
/*Channel 3   */
/*Channel 4   */
/*Channel 5   */
/*Channel 6   */
/*Channel 7   */
/*Channel 8   */
/*End point adjustment*/
/*End point switch */
/*Fail-safe */
/*Channel 1   */
/*Channel 2   */
/*Channel 3   */
/*Channel 4   */
/*Channel 5   */
/*Channel 6   */
/*Channel 7   */
/*Channel 8   */
/*Acceleration */
/*Neutral */
/*Forward */
/*Brake1 */
/*Brake2 */
/*Brake3 */
/*Channel limiter */
/*Double Ratio */
/*Ratio Switch*/
/*Steering rate */
/*Switch select */
/*Brake rate */
/*OFF */
/*ON */
/*Idle up */
/*Status */
/*Trim switch */
/*Function switch */
/*Idle up rate */
/*OFF */
/*NULL */
/*Steering */
/*Throttle */
/*Rotary knob */
/*DT1 */
/*DT2 */
/*DT3 */
/*DT4 */
/*DL1 */
/*PS1 */
/*PS2 */
/*PS3 */
/*PS4 */
/*PS5 */
/*Streering switch */
/*Trigger switch */
/*Steering 2 */
/*Wheel to left */
/*Wheel to right */
/*Dual ESC 1 */
/*Dual ESC 2 */
/*4WS steering1 */
/*4WS steering2 */
/*Tilt steering */
/*Tilt flap */
/*CPS mixing1 */
/*CPS mixing2 */
/*CPS mixing3 */
/*CPS mixing4 */
/*Brake 2 */
/*Brake 3 */
/*Gyro mixing */
/*Channel setting */
/*Channel 1   */
/*Channel 2   */
/*Channel 3   */
/*Channel 4   */
/*Channel 5   */
/*Channel 6   */
/*Channel 7   */
/*Channel 8   */
/*--------- */
/*Receiver signal */
/*Receiver voltage */
/*Transmitter voltage */
/*EXT voltage */
/*Current sensor */
/*RPM sensor */
/*Temperature */
/*GPS */
/*Sensor list */
/*Sensor list1 */
/*Sensor list2 */
/*Sensor list3 */
/*Sensor list4 */
/*Sensor list5 */
/*Sensor list6 */
/*Sensor list7 */
/*Previous */
/*Next */
/*Sensor setting */
/*Sensor setting1 */
/*Sensor setting2 */
/*Sensor setting3 */
/*Sensor setting4 */
/*Sensor setting5 */
/*Sensor setting6 */
/*Sensor setting7 */
/*Previous */
/*Next */
/*Receiver signal */
/*Current signal */
/*Minimum */
/*Alarm sound type */
/*Vibration type */
/*Alarm limit */
/*Alarm interval */
/*Buzzer */
/*Inhibit */
/*Mode1 */
/*Mode2 */
/*Mode3 */
/*Inhibit */
/*xxx voltage */
/*Current voltage */
/*Minimum */
/*Alarm sound type */
/*Vibration type */
/*Alarm voltage */
/*Alarm interval */
/*Buzzer */
/*Inhibit */
/*Receiver voltage */
/*Engine battery voltage */
/*Mode1 */
/*Mode2 */
/*Mode3 */
/*Inhibit */
/*xxx sensor */
/*Current data */
/*Maximum */
/*Alarm sound type */
/*Vibration type */
/*Limit */
/*Minimum */
/*Alarm sound type */
/*Vibration type */
/*Limit */
/*Buzzer */
/*Inhibit */
/*Voice */
/*Vibration1 */
/*Inhibit */
/*Mode1 */
/*Mode2 */
/*Mode3 */
/*Telemetry broadcast*/
/*Auto */
/*Switch */
/*Broadcast interval */
/*Stop broadcast button*/
/*EXP */
/*VTR */
/*Multiple point */
/*Steering curve */
/*Type */
/*Quick/Slow */
/*EXP rate */
/*Fine tune(left) */
/*Fine tune(right) */
/*VTR point */
/*Quick */
/*Slow */
/*EXP */
/*VTR rate */
/*VTR */
/*Throttle curve */
/*Type */
/*Rate */
/*Quick/Slow */
/*EXP rate */
/*Quick */
/*VTR rate */
/*Point */
/*Slow */
/*Brake curve */
/*Brake curve1 */
/*Brake curve2 */
/*Brake curve3 */
/*Quick/Slow */
/*EXP rate */
/*Quick */
/*VTR rate */
/*Point */
/*Slow */
/*Brake curve */
/*Type */
/*Rate */
/*Steering delay*/
/*Turn */
/*Return */
/*Throttle delay*/
/*Mode */
/*Turn*/
/*Return*/
/*High */
/*Middle */
/*Low */
/*Point1 */
/*Point2 */
/*All mode */
/*All point */
/*High-Low point */
/*Three point */
/*Traction control */
/*Mixing */
/*Throttle return */
/*Delay */
/*Cycle speed */
/*Interval rate */
/*Trigger point */
/*Trigger mode */
/*ON */
/*OFF */
/*Normal */
/*Reverse */
/*A.B.S. */
/*A.B.S.1 */
/*A.B.S.2 */
/*A.B.S.3 */
/*A.B.S. */
/*A.B.S. */
/*Steering trigger */
/*Brake channel */
/*Brake return */
/*Delay */
/*Cycle speed */
/*Interval rate */
/*ST trigger to start */
/*A.B.S trigger to start */
/*Trigger mode */
/*ON */
/*OFF */
/*CH2 */
/*Normal */
/*Reverse */
/*Throttle start */
/*Mode switch */
/*Trigger point */
/*Preset point */
/*Status */
/*Trigger point */
/*Preset point */
/*Ready */
/*Switch select */
/*OFF */
/*Trigger */
/*Engine cut */
/*Mode Switch */
/*Switch select */
/*Preset point */
/*Status */
/*Preset point */
/*Ready */
/*OFF */
/*Trigger */
/*Steering mixing */
/*Mixing */
/*Ackermann */
/*Rate */
/*Left */
/*Right */
/*Steering1 */
/*Steering2 */
/*Left */
/*Right */
/*Left */
/*Right */
/*ST1 */
/*ST2 */
/*ST CH1 */
/*ST CH2 */
/*Switch */
/*Brake rate */
/*CH1 */
/*CH5 */
/*Brake mixing */
/*Brake1 */
/*Brake2 */
/*Brake3 */
/*Brake channel */
/*Brake rate */
/*Brake delay */
/*ST mixing(left) */
/*ST mixing(right) */
/*Brake2/3 rate */
/*CH2 */
/*CH7 */
/*CH8 */
/*Gyro mixing */
/*Mixing */
/*Channel */
/*Gyro type */
/*CH1 */
/*Gyro built-in */
/*Gyro gain */
/*Group1 */
/*Gain1 */
/*Gain2 */
/*Normal */
/*Group2 */
/*Gain3 */
/*Gain4 */
/*Normal */
/*Gyro mixing */
/*Current gain */
/*Gain switch */
/*Gain group type switch */
/*Gain type switch */
/*Gyro mixing switch */
/*Group1 */
/*Gain1 */
/*Gyro built-in */
/*Gain1 */
/*Gain2 */
/*Gain4 */
/*Gain3 */
/*NULL */
/*Group1 */
/*Group2 */
/*Normal */
/*AVCS */
/*4WS mixing */
/*Mixing */
/*MIX mode */
/*4WS type */
/*4WS CH1 */
/*4WS CH2 */
/*CH1 rate */
/*CH2 rate */
/*Mode1 */
/*CH1 */
/*CH2 */
/*ST1 */
/*ST2 */
/*4WS mixing */
/*Switch select */
/*Front rate */
/*Rear mix rate */
/*Mode change */
/*Front */
/*Reverse */
/*Same */
/*Rear */
/*Type1 */
/*Type2 */
/*Type3 */
/*Type4 */
/*Dual ESC mixing */
/*Mixing */
/*MIX mode */
/*Trim mode */
/*ESC1 channel */
/*ESC2 channel */
/*ESC1 rate */
/*ESC2 rate */
/*CH1 */
/*CH2 */
/*Dual ESC mixing */
/*Switch select */
/*Dual ESC switch */
/*Drive rate */
/*Dual ESC(front) */
/*Dual ESC(4WD) */
/*Dual ESC(rear) */
/*CPS mixing */
/*CPS mixing1 */
/*CPS mixing2 */
/*CPS mixing3 */
/*CPS mixing4 */
/*CPS mixing */
/*Mixing */
/*Trigger CH */
/*Operation CH */
/*Trigger mode */
/*Point1 */
/*Point2 */
/*Point3 */
/*Point4 */
/*Operation mode */
/*Cycle speed */
/*Point1 */
/*Point2 */
/*CH1 */
/*CH8 */
/*Neutral */
/*Off till triggered to flash */
/*Function switch */
/*Neutral */
/*Left */
/*Right */
/*Both sides */
/*PS switch */
/*Off till triggered to flash */
/*Flash till triggered to off */
/*Off till triggered to on */
/*On till triggered to off */
/*CPS mixing */
/*Tank mixing */
/*Mixing */
/*Mixing channel */
/*Mixing rate */
/*Left */
/*Right */
/*Forward limit */
/*Back limit */
/*Forward */
/*Back */
/*Left */
/*Right */
/*CH1 */
/*CH2 */
/*Tilt mixing */
/*Mixing */
/*CH1 */
/*CH2 */
/*CH1 rate */
/*CH2 rate */
/*Flap */
/*Rudder to flap */
/*Flap to rudder */
/*CH1 */
/*CH2 */
/*CH1 */
/*CH2 */
/*EXP */
/*VTR */
/*Multiple point */
/*Tilt mixing */
/*Switch select */
/*Flap */
/*RUD->FLP */
/*FLP->RUD */
/*Program. mixing */
/*Program. mixing1 */
/*Program. mixing2 */
/*Program. mixing3 */
/*Program. mixing4 */
/*Program. mixing5 */
/*Program. mixing6 */
/*Program. mixing7 */
/*Program. mixing8 */
/*Program. mixing1 */
/*Curve type */
/*Quick/Slow */
/*Offset */
/*Curve rate */
/*EXP rate */
/*Fine tune(L) */
/*Fine tune(R) */
/*Mixing rate */
/*Left */
/*Right */
/*Slow */
/*Program. mixing1 */
/*Curve type */
/*Quick/Slow */
/*Offset */
/*Point */
/*Curve rate */
/*VTR rate */
/*Fine tune(L) */
/*Fine tune(R) */
/*Mixing rate */
/*Left */
/*Right */
/*Slow */
/*Program. mixing1 */
/*Curve type */
/*Offset */
/*Point rate */
/*Multiple point */
/*Program. mixing1 */
/*Switch select */
/*Mixing */
/*MIX mode */
/*Trim mode */
/*Mixing channel */
/*Master */
/*Slave */
/*Throttle */
/*Steering */
/*Program. mixing */
/*Quick */
/*Slow */
/*Last */
/*Next */
"/*occupying this channel!

Do you want to replace it? */"
/*YES */
/*NO */
"/*occupies this button!

Do you want to replace it? */"
/*Input output mode*/
/*Video input Settings*/
/*Luminance*/
/*Contrast*/
/*Saturability*/
/*Hue*/
/*No operation*/
/*Warning*/
/*Alarm time*/
/*Alarm type*/
/*Auto OFF*/
/*OFF time*/
/*Null*/
/*Buzz*/
/*Voice*/
/*Model name conflict*/
/*Please power off the receiver first to avoid accidents!*/
/*Do you want forced shutdown?*/
/*Return*/
/*Minimum*/
/*Median*/
/*Maximum*/
/*Quick setup*/
"/*!""""#$%&'()*+,-./
0123456789:;<=>?
@ABCDEFGHIJKLMNO
PQRSTUVWXYZ[\]^_
`abcdefghijklmno
pqrstuvwxyz{|}~
*/"
/*Servo Speed*/
/*Model Interaction*/
/*Multi-protocol output switch*/
/*Manual Download Address:*/
